Acute Experiment Arduino Commands

|  |  |  |
| --- | --- | --- |
| Command | Function | Default |
| L | Toggle Local Probing On/Off | Off |
| K/J/H | Set local probing level (Low/Middle/High) | Middle |
| G | Toggle Global Mid-level On/Off | Off |
| F | Toggle global mid-level+local probing | Off |
| S | Switch context |  |
| T | Cycling On | On (5 min/block) |
| I | Cycling Off |
| P | Auto Probing On (2 min / 5 min block) | Off |
| C | Auto Probing Off (coupling) |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |