Acute Experiment Arduino Commands

|  |  |  |
| --- | --- | --- |
| Command | Function | Default |
| L | Manually Toggle Local Probing On/Off | Off |
| H/J/K | Set local probing level (H=-1/J=0/K=+1) | 0 |
| S | Switch context A/B | A |
| C | Switch Context source chin/trunk | chin |
| P | Pairing (10 min cycling) | ON |
| R | Sporadic probing (5 min cycling, 1/10 probing) | Off |
| T | Auto Probing (5 min cycling, 1st and last 1.25 probing) | Off |
| I | Cycling Off | Off |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |